**Daily PPE Inspection Checklist**  
*For use by on-site inspectors to verify worker compliance with PPE requirements.*

**Worker Name:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **Date:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  
**Inspector Name:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |  |
| --- | --- |
| **1. Hard Hats**  ☐ No visible cracks, dents, or damage. ☐ Worn properly (bill forward, snug fit). ☐ Chin strap used (if required).  **2. Safety Glasses/Goggles**  ☐ Free from scratches, cracks, or damage. ☐ Worn in designated areas (e.g., cutting, grinding). ☐ Properly fitted (no slipping, covers eyes fully).  **3. Gloves**  ☐ Appropriate type for the task (e.g., cut-resistant, chemical-resistant). ☐ No tears, holes, or excessive wear. ☐ Properly sized for comfort and safety.  **4. High-Visibility Vests**  ☐ Clean and reflective strips intact. ☐ Worn at all times on-site. ☐ Proper fit (not too loose or tight).  **5. Steel-Toe Boots**  ☐ Proper fit and in good condition (no cracks or holes). ☐ Non-slip soles intact. ☐ Laces or straps secured to prevent tripping. | **6. Hearing Protection**  ☐ Earplugs or earmuffs available. ☐ Worn in high-noise areas (e.g., machinery, power tools). ☐ Properly fitted (earplugs inserted correctly, earmuffs snug).  **7. Respirators/Masks (if required)**  ☐ Correct type for the hazard (e.g., dust, fumes). ☐ Proper fit and seal (no gaps). ☐ Filters/cartridges in good condition and not expired.  **8. Fall Protection (if required)**  ☐ Harness and lanyard inspected for damage. ☐ Properly worn and adjusted (straps snug, D-ring centered). ☐ Anchorage point verified and secure.  **9. Additional PPE (if required)**  ☐ Face shields (used with safety glasses, no damage). ☐ Knee pads (properly fitted, no damage). ☐ Coveralls/protective clothing (appropriate for task, no tears). |

**Inspector Notes:**

* Any issues observed (e.g., damaged PPE, non-compliance):
* Corrective actions taken:

**Worker Signature:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  
**Inspector Signature:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_